The modified 4 node circuit with the IM placed at bus 4 is shown below

A diagram of a load

Description automatically generated

Fault occurs at bus 4 at t = 0.0833 s and lasts for 0.3333 s until t = 0.4167 where it clears.

A graph of a graph

Description automatically generated